**Additional Requirements for Workshops, Fieldwork and Laboratories**

**Examples of Standards applying to Electrical Equipment**

| **Electrical Equipment** | **Example** |
| --- | --- |
| Single Phase RCD protected EPOD minimum IP rating of IP 33  Minimum standard for hostile use in field work, or energised from generator (non-mains power source) | Renegade Industrial 10Amp RCD 4 Outlet Power Board |
| 3 Phase Plug into Single phase outlets RCD protected | Image result for industrial power board pictures |
| 3 Phase Plug with 3 Phase outlets with RCD protection | Related image |
| Light Duty 240V 10A Extension Lead for non-hostile areas such as Office spaces only | Image result for Australian standards on electrical extension leadsImage result for Australian standards on electrical extension leads |
| 25m 240V 15A Heavy Duty lead, can also get in 10A heavy duty  For workshops and fieldwork  **NOTE:** 25M is the max length for any extension lead | Image result for Australian standards on electrical extension leads |
| Double Adaptors - **NOT FOR USE** anywhere on University property | Image result for double adaptorsImage result for double adaptors |